(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "TMC2209_SILENTSTEPSTICK"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U9"
			(at 0 25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "TMC2226"
			(at 0 22.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "TMC2209_SILENTSTEPSTICK:MODULE_TMC2209_SILENTSTEPSTICK"
			(at -3.556 -26.416 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "TMC2209_SILENTSTEPSTICK_0_0"
			(rectangle
				(start -12.7 20.32)
				(end 12.7 -20.32)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "~{EN}"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "STEP"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "DIR"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "MS1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "MS2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "VIO"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "VM"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 17.78 0 180)
				(length 5.08)
				(name "M1A"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "M2B"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(symbol "TMC2209_SILENTSTEPSTICK_1_0"
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "UART"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "CLK"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "STDBY"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "DIAG"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "VREF"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "M2A"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "M1B"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
)
