
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "MMC5603NJ" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 8.382 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "MMC5603NJ" (id 1) (at -10.16 -10.16 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "MMC5603NJ:XDCR_MMC5603NJ" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Memsic Inc." (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "0.6 mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "UFBGA-4 Memsic Inc." (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/MMC5603NJ/Memsic+Inc./view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "B" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/MMC5603NJ/Memsic+Inc./view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "MMC5603NJ" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            Magnetoresistive Sensor X, Y, Z Axis 4-WLP (0.82x0.82)\n                        \n" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SNAPEDA_PN" "MMC5603NJ" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Memsic Inc." (id 16) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "MMC5603NJ_0_0"
      (rectangle (start -10.16 -7.62) (end 10.16 7.62)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at 15.24 -5.08 180.0) (length 5.08)
        (name "VSA"
          (effects (font (size 1.016 1.016)))
        )
        (number "A1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 5.08 180.0) (length 5.08)
        (name "VDD"
          (effects (font (size 1.016 1.016)))
        )
        (number "B1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input clock (at -15.24 2.54 0) (length 5.08)
        (name "SCL"
          (effects (font (size 1.016 1.016)))
        )
        (number "A2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 0.0 0) (length 5.08)
        (name "SDA"
          (effects (font (size 1.016 1.016)))
        )
        (number "B2"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)